70824 - Column – deck-mounted mixer – rinsing head
Single hole deck-mounted column with hand shower and filling spout. Single-lever mixer with ceramic head 1/4 turn with flow rate of 26L / min at 3 bar, with chromed brass column and body, flexible, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm. Hand shower M 1/2 '' black with 2 adjustable jets; Stainless steel braided shower hose Lg 1 m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max. Flexible PEX - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves. Adjustable spout projection 340 mm. Reference 70824, PRESTO brand or equivalent.

70824 - Column – deck-mounted mixer – rinsing head
Single hole deck-mounted column with hand shower and filling spout. Reference 70824, PRESTO brand or equivalent, including:
- Single-lever mixer with ceramic head 1/4 turn with flow rate of 26L /min at 3 bar, with column and body in chromed brass, flexible, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm
- M 1/2 '' black hand shower with 2 adjustable jets; Stainless steel braided shower hose Lg 1 m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max
- PEX hoses - stainless steel braid G 1/2 '' 660 mm,
- Integrated NF check valves
- Adjustable spout 340 mm projection