70828 - Wall-mounted column with 2 holes – rinsing head
Two-hole deck-mounted column with hand shower and filling spout. Two-hole mixer on deck with 1/4 turn ceramic head with flow rate of 37L / min at 3 bar, with brass column and body, flexible hose, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm. Hand shower M 1/2 '' black with 2 adjustable jets; Stainless steel braided shower hose Lg 1m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max. Flexible PEX - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves. Adjustable spout projection 340 mm. Reference 70828, PRESTO brand or equivalent.

70828 - Wall-mounted column with 2 holes – rinsing head
Two-hole deck-mounted column with hand shower and filling spout. Reference 70828, PRESTO brand or equivalent, including:
- Two-hole mixer on deck with 1/4 turn ceramic head with flow rate of 37L /min at 3 bar, with brass column and body, flexible hose, stainless steel spring and wall mounting bracket, can be cut from 60 to 200 mm
- M 1/2 '' black hand shower with 2 adjustable jets; Stainless steel braided shower hose Lg 1m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max
- Flexible PEX - stainless steel braid G 1/2 '' 660 mm
- Integrated NF check valves
- Adjustable spout 340 mm projection