70830 - « Mini » Column –deck-mounted mixer -rinsing head
Single hole deck-mounted column with hand shower and filling spout. Overall height: 764 mm. Single-lever mixer with ceramic head 1/4 turn with flow rate of 26L / min at 3 bar, with brass column and body, flexible, stainless steel spring. Hand shower M 1/2 '' black with 2 adjustable jets; Stainless steel braided shower hose Lg 1 m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max. PEX hoses - stainless steel braid G 1/2 '' 660 mm, integrated NF non-return valves. Adjustable spout 250 mm projection. Reference 70830, PRESTO brand or equivalent

70830 - « Mini » Column –deck-mounted mixer -rinsing head
Single hole deck-mounted column with hand shower and filling spout. Overall height: 764 mm. Reference 70830, PRESTO brand or equivalent, including:
- Single-lever mixer with ceramic head 1/4 turn with flow rate of 26L / min at 3 bar, with brass column and body, flexible, stainless steel spring.
- M 1/2 '' black hand shower with 2 adjustable jets; Stainless steel braided shower hose Lg 1 m surrounded by a PU sheath resistant to temperatures up to 90 ° C. Continuous operating temperature at 70 ° C max
- PEX hose - stainless steel braid G 1/2 '' 660 mm.
- Integrated NF check valves
- Adjustable spout 250 mm projection