70832 - Special ' Under Counter ' Bar- Deck-mounted mixer tap
Single-lever deck-mounted mixer with upward spout. Special bar application with spout under the counter. Swivel spout, projection 250 mm, height under spout 146 mm, diameter 22 mm. Ceramic cartridge with flow rate of 25L / min at 38°C at 3 bar. Anti-limescale star-shaped flow straightener. Supply by PEX flexible hose - G1 / 2 '' braid Lg 660 mm, resistant to temperatures up to 90 ° C. Integrated NF check valves. Chromed brass body and spout. Reference 70832, PRESTO brand or equivalent.

70832 - Special ' Under Counter ' Bar- Deck-mounted mixer tap
Single-lever deck-mounted mixer with upward spout. Special bar application with spout under the counter, reference 70832, brand PRESTO or equivalent, including:
- Swivel spout, projection 250 mm, height under spout 146 mm, diameter 22 mm
- Ceramic cartridge with flow rate of 25L / min at 38°C at 3 bar.
- Anti-limescale star-shaped flow straightener
- Supply by PEX flexible hose - stainless steel braid G1 / 2 '' Lg 660 mm, resistant to temperatures up to 90 ° C
- Integrated NF non-return valves
-Chromed brass body and spout