70834 - Lateral control – Deck-mounted mixer tap – upward spout
Single-lever deck-mounted mixer with upward spout. Control at the side elbow. Swivel spout, projection 250 m, height under spout 276 mm, diameter 22 mm. Ceramic cartridge with flow rate of 25L / min at 38°C at 3 bar. Anti-tartar spray breaker. Supply by PEX hose - stainless steel braid G1 / 2 '' Lg 660 mm. Flexible resistant to temperatures up to 90 ° C. Integrated NF check valves. Chromed brass body and spout. Reference: 70834 PRESTO brand, or equivalent.

70834 - Lateral control – Deck-mounted mixer tap – upward spout
Single-lever deck-mounted mixer with upward spout and side elbow control, reference 70834 of PRESTO brand, or equivalent, comprising:
- Swivel spout, projection 250 m, height under spout 276 mm, diameter 22 mm
- Ceramic cartridge with flow rate of 25L / min at 38°C at 3 bar
- Supply by PEX hose - stainless steel braid G1 / 2 '' Lg 660 mm. Flexible hose resistant to temperatures up to 90 ° C
- Integrated NF check valves
- Chromed brass body and spout