75025 - Hospital washbasin mixer with fixed spout no drain
Single hole washbasin mixer without drain for handwash basin, deck-mount with solid handle. Fixed cast spout L 115mm. Height to nozzle 55mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 13.8l/min. Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M12x1, LN G'3 / 8 L 350mm Reinforced fixation by a stainless steel rod. 10 year warranty. Sanifirst brand single hole washbasin mixer, fixed cast spout REF: 75025 or approved equivalent.