75049 - Hospital washbasin mixer, fixed spout and drain
Single hole washbasin mixer with brass handwash basin drain, deck-mount with solid handle. Fixed tall cast spout L 110mm. Height to nozzle 82mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow (hard point at 50% opening). Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min.Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M10x1 LN G'3 / 8 L 350mm Reinforced fixation by a stainless steel rod. Basket filter seals mounted on the hoses limiting fouling.10 year warranty. Sanifirst brand single hole washbasin mixer, tall fixed cast spout REF: 75049 or approved equivalent.