75070 - Hospital sink mixer, swivel spout, with extractable shower head
Single hole sink mixer deck-mount with solid handle. Swivel spout and two-spray shower head with removable limescale spikes and sliding hose. Height to nozzle 126mm, L 210mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow (hard point at 50% opening). Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Tapware fitted as standard star-shaped flow straightener. Body, spout, shower head and controls in polished chrome plated brass. SPEX Hoses, M10x1 LN G'3 / 8 L 350mm. Basket filter seals mounted on the hoses limiting fouling. Reinforced fixation by a stainless steel rod. 10 year warranty. Sanifirst brand single hole sink mixer, swivel spout and retractable shower head REF: 75070 or approved equivalent.