75072 - Hospital shower mixer - Full lever
Shower mixer, 150mm span, no drain , wall-mount with solid handle . Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow (hard point at 50% opening). Flow between 9 and 12L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 9 and 20L / min.Body and control in polished chrome plated brass. Shower outlet M G'1 / 2 with integrated back-flow valve. Connection LN G'3 / 4 comes with rosettes and off-centre fittings M G’1/2 10 year warranty. Sanifirst brand shower mixer, 150mm span REF: 75072 or approved equivalent.