75073 - 
Shower mixer, 150mm span, wall-mount with solid handle Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 13.8l/min. Body and control in polished chrome plated brass. Shower outlet M G'1 / 2 with integrated back-flow valve. Connection LN G'3 / 4
comes with rosette cover plates and off-centre fittings M G'1 / 2 and 1 spray chrome shower head anti-scaling system; metal plastic 1.5m hose and 25 mm diameter bar l 600mm. 10 year warranty. Sanifirst brand shower mixer, 150mm span REF: 75073 or approved equivalent.