75079 - Hospital sink mixer, wall-mount, with downward spout, swivel
Single hole sink mixer, wall-mount with solid upward handle. Smooth tube downward spout, swivel L 200mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 13.8l/min. Tapware fitted as standard star-shaped flow straightener. Smooth body, spout and controls in polished chrome plated brass. SPEX Hoses, M10x1 LN G'3 / 8 L 350mm Reinforced fixation by a stainless steel rod. 10 year warranty. Sanifirst brand single hole sink mixer, wall mount, downward, smooth tube spout and upward pointable handle REF: 75079 or approved equivalent.