75112 - Hospital thermostatic shower mixer, thermal shock - Mastermix 
Thermostatic shower mixer MASTERMIX design equipped with ergonomic downward flow control handle.
Temperature knob locked at 38 ° C (Secured release for thermal shock accessible only by technical services without need to remove knob.)
150mm span, off centre M 1/2 fittings with chrome cover plates and filter seals. Shower output M'1 / 2 downward with integrated back-flow valve. Adjustable flow rate between 5 and 14l/min, adjustable temperature from 18 to 38 ° C. 
Unique patented system avoiding communication between hot and cold water supplies eliminating back-flow valves on mixer supplies using a ceramic cartridge and a thermostatic cartridge NF EN 111.
3-year warranty for the thermostatic cartridge and 10-year warranty for the rest of the fittings.  PART NO.: 75112, MASTERMIX design, Sanifirst brand or approved equivalent..