75120 - Hospital wall-mount washbasin mixer with fixed spout no drain
Single hole washbasin mixer, no drain, wall-mount for hand wash basin, with 157mm long medical handle avoiding manual contact, using elbow, forearm or wrist. Smooth tube spout, fixed and removable L 200mm. Multifunction ceramic cartridge Ø 35: 7-setting temperature limit stop, flow settings from 2l to 13.8l/min. Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M10x1 LN G'3 / 8 L 350mm Reinforced fixation by a stainless steel rod. 10 year warranty. Sanifirst brand single hole washbasin mixer, wall-mount, fixed smooth tube spout REF: 75120 or approved equivalent.