75128 - Hospital mixer, fixed or adjustable spout, removable - Modul'Mix
Single hole hospital mixer (Modul'mix design), no drain, for hand wash basin, with 220mm long medical handle avoiding manual contact, using elbow, forearm or wrist. Fixed or swivel spout, smooth and removable for disinfecting L 200mm. Height to nozzle 100mm. Height and length of spout adapted without changing the entire tapware. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop,dual flow (hard point at 50% opening). Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Tapware with star-shaped flow straightener, eliminating water retention and impurities; withstands thermal and chlorine shocks Smooth body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M10x1 LN G'3 / 8 L 500mm Reinforced fixation by a stainless steel rod. 10 year warranty. Chlorine and thermal shock resistant. Certified NF Medical classification. Sanifirst brand hospital mixer, fixed or swivel smooth spout, removable, for hand wash basin REF: 75128 or approved equivalent.