75136 - 
Single hole hospital mixer (Modul'mix design), no drain, for hand wash basin, with 220mm long medical handle avoiding manual contact, using elbow, forearm or wrist. Fixed or swivel spout, smooth and removable for disinfecting L 200mm. Height to nozzle 200mm. Height and length of spout adapted without changing the entire tapware. Ceramic cartridge Ø 40, pressure balancing: 7-setting temperature limit stop, dual flow (hard point at 50% opening). Flow between 10 and 15L / min at 3 bar. Integrated check valves. Tapware with star-shaped flow straightener eliminating water retention and impurities; withstands thermal and chlorine shocks Smooth body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M10x1 LN G'3 / 8 L 650mm Reinforced fixation by a stainless steel rod. 10 year warranty. . Sanifirst brand hospital mixer, single hole and pressure balancing, fixed or swivel smooth spout, removable, for hand wash basin REF: 75136 or approved equivalent.