75149 - Electronic mixer, mains powered, fixed or adjustable  removable nozzle, - Modul'Mix
Electronic mains powered single hole mixer without drain, comes with chrome short control for temperature setting (long handle available on request). Fixed or adjustable spout, smooth and removable for disinfecting L 250mm. Height to nozzle 100mm suitable for end filtration. Height and length of spout adapted without changing the entire tapware. Multifunctional cartridge: temperature limit stop with 7 positions adjustment; and flow blocked between 4 and 6L / min at 3 bar in accordance with NF "Medical Environment", possible flow modification, in case of disassembly of the limiters, between 4 and 20L / min.Infrared cell integrated in the body, removable without removing the tap. Electronic housing, mains 220V input, 6V output. Tapware fitted as standard star-shaped flow straightener. Smooth body, spout and controls in polished chrome plated brass. SPEX stainless steel hoses, M10X1, LN G'3 / 8 L 500 mm, filters, solenoid valves and silicon membrane M G'3 / 8. Reinforced fixation by a stainless steel rod. 3 year warranty. Chlorine and thermal shock resistant. Customisable anti-bacteria program (purges, frequency, duration, etc.). Sanifirst brand mains powered single hole electronic mixer, fixed and removable spout REF: 75149 or approved equivalent.