75421 - Single lever washbasin mixer -  Without  drain - Cast spout 119 x 53,5mm
Single-hole deck-mounted washbasin mixer tap with NF plastic drainage with solid control. Cast, fixed spout, Len 19 mm. Spout height 53.5 mm. Ø 40 multi-function ceramic cartridge: temperature limiting stopper with 7 setting positions, double flow and maximum flow settings. Tapware fitted with water saving aerator as standard. Body, spout and control component in polished chrome-plated brass. Hoses with SPEX sheath braided stainless steel M12X1, EP G’3/8, Len 370 mm. Fixture strengthened using an M8 rod. 10 year guarantee. Sanifirst brand type single hole washbasin mixer tap fixed with cast spout REF: 75421 or approved equivalent.