75549 - 
Shower mixer, 150mm span, no drain , wall-mount with long openwork handle Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 13.8l/min. Body and control in polished chrome plated brass. Shower outlet M G'1 / 2 with integrated back-flow valve. Connection LN G'3 / 4 comes with rosettes and off-centre fittings M G’1/2. Shower mixer with 2-jet spray head (reference 75280), hose (reference 75280), and chrome-plated 25 mm diameter shower rail length 600 mm with soap-holder (reference 75288).