75615 - Hospital washbasin mixer with fixed spout no drain
Single hole washbasin mixer without drain for hand wash basin, deck-mount with 157mm long medical handle avoiding manual contact, using elbow, forearm or wrist. Fixed cast spout L 119mm. Height to nozzle 53.5mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow (hard point at 50% opening). Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M12x1, LN G'3 / 8 L 350mm. Basket filter seals mounted on the hoses limiting fouling. Reinforced fixation by a stainless steel rod. 10 year warranty. Sanifirst brand single hole washbasin mixer, fixed cast spout REF: 75615 or approved equivalent.