75617 - Single hole washbasin mixer tap - Energy savings -without drainage
Single-hole deck-mounted hand-basin mixer tap without drainage, with thin control. Fixed cast spout projection 100.5mm. Spout height 92mm. Ø 35 energy saving ceramic cartridge: opening on cold water, with temperature limit limiter, allowing 9-position adjustment.. Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min.  Tapware fitted with star-shaped flow straightener as standard. Body, spout and control component in polished chrome-plated brass. Hoses with SPEX sheath braided stainless steel M10X1, EP G’3/8, Len 500mm. Basket filter seals mounted on the hoses limiting fouling. Fixture strengthened using an M8 rod. 10 year guarantee. Sanifirst brand type single hole washbasin mixer tap with fixed cast spout REF: 75617 or approved equivalent.