75623 - 
Single-hole deck-mounted sink mixer tap without drainage, with wire control. Directional spout. Spout height 220mm. Projection 169mm. Ø 40 multi-function ceramic cartridge: 7-setting temperature limit stop, dual flow (hard point at 50% opening). Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Tapware fitted with star aerator as standard. Body, spout and control component in polished chrome-plated brass. SPEX hoses M10X1, EP G 3/8”, Len 400mm. Basket filter seals mounted on the hoses limiting fouling. Fixture strengthened using an M8 rod. 10 year guarantee. Sanifirst brand type single hole sink mixer tap with directional spout REF: 75623 or approved equivalent.