75624 - Sink mixer tap with extractable hand spray 
Single-hole deck-mounted sink mixer tap without drainage, with wire control. Directional spout and extractable 2-position hand spray (anti-splay-nozzle, rain).  Spout height 195mm. Projection 196mm. Ø 40 multi-function ceramic cartridge:7-setting temperature limiter, dual flow (hard point at 50% opening). Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Tapware fitted with star-shaped flow straigthener M24 X 100 as standard. Body, spout, hand-spray and control component in polished chrome-plated brass. M10 X 1 hoses EP G’3/8 Length 450 mm SPEX. Basket filter seals mounted on the hoses limiting fouling. Fixture strengthened by a drum. 10 year guarantee. Sanifirst brand type single hole sink mixer tap with directional spout REF: 75624 or approved equivalent