75627 - 
Sink mixer, 150 mm span, without drain, wall mount with 170mm long medical handle avoiding manual contact, using elbow, forearm or wrist. Swivel cast spout L 200mm. Multifunction ceramic cartridge Ø 40: 7-setting temperature limit stop, dual flow and flow settings from 2l to 13.8l/min. Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. Connection LN G'3 / 4 comes with rosettes and off-centre fittings M G’1/2 10 year warranty. Sanifirst brand single hole sink mixer, 150 mm span, swivel, cast spout REF: 75627 or approved equivalent.