75631 - 
Thermostatic single hole washbasin mixer, no drain, for hand wash basin, deck-mount. Swivel and removable cast spout L 169mm. Height to nozzle 164mm. Dual flow control knob and a special heat shock knob locked at 38 ° C and 41°with a secure release system for thermal shock without changing knob and accessible only by technical services. ½ turn ceramic head for flow control and NF Thermostatic cartridge for adjusting the temperature. Tapware fitted as standard star-shaped flow straightener. Body, spout and knobs in polished chrome-plated brass. SPEX stainless steel braided hoses, M10x1 LN G'3 / 8 L 385 mm Reinforced fixation by a stainless steel rod. 3-year warranty for the thermostatic cartridge and 10-year warranty for the rest of the fittings. Sanifirst brand single hole washbasin mixer, swivel cast spout REF: 75631 or approved equivalent.