75634 - Single lever washbasin mixer -  With  drain - Cast spout 110 x 78,5mm
Single-hole deck-mounted washbasin mixer tap with brass drainage and solid control. Fixed high cast spout Len 110mm. Spout height 78.5 mm. Ø 40 multi-function ceramic cartridge: temperature limiting stopper with 7 setting positions, double flow and maximum flow settings. Tapware fitted with water saving aerator as standard. Body, spout and control component in polished chrome-plated brass. Hoses with SPEX sheath braided stainless steel M10X1, EP G’3/8, Len 350mm (Len 450 mm from 2016). Fixture strengthened using an M8x rod. 10 year guarantee. Sanifirst brand type single hole washbasin mixer tap with fixed high cast spout REF: 75634 or approved equivalent.