75635 - Single lever washbasin mixer ECO C3 -  With  drain - Cast spout 110 x 92mm
Single-hole deck-mounted washbasin mixer tap with NF plastic drainage for hand-basin with thin control. Fixed cast spout projection 100.5mm. Spout height 92mm. Ø 35 energy saving ceramic cartridge: opening on cold water, hard spot at 3.9L/min at 3 bars. Tapware fitted with water saving aerator as standard. Body, spout and control component in polished chrome-plated brass. Hoses with SPEX sheath braided stainless steel M10X1, EP G’3/8, Len 500mm. Fixture strengthened using an M8 rod. 10 year guarantee. Sanifirst brand type single hole washbasin mixer tap with fixed cast spout REF: 75635 or approved equivalent