75638 - Hospital thermostatic shower mixer
Wall mounted thermostatic shower mixer 150 mm center distance, cold body. A long brass control for opening and a knob with temperature stop at 38 ° C. Possibility of going up to 48 ° C. Flow rate of 14.4L / min at 3 bar. Pair of sheet metal rosette and eccentric connection G'1 / 2 G'3 / 4 and filter gaskets. DCW / DHW inlet fitted with check valve, M'1 / 2 shower outlet. 1/4 turn ceramic head for flow rate adjustment and thermostatic cartridge conforming to NF EN 1111 for temperature adjustment. Body and maneuvering knobs in polished chrome-plated brass. Warranty 3 years for the thermostatic cartridge and 10 years for the rest of the mixer. Sanifirst brand thermostatic shower mixer type 150 mm center distance REF: 75638 or approved equivalent.