75639 - Hospital thermostatic shower mixer, thermal shock
150mm span thermostatic wall-mount shower mixer Dual flow control knob and a special heat shock knob locked at 38 ° C and 41°C with a secure release system for thermal shock without changing knob and accessible only by technical services. Off centre M 1/2 fittings with chrome cover plates and filter seals. Hot and cold water supplies equipped with back-flow valves, shower outlet M'1 / 2. ½ turn ceramic head for flow control and NF Thermostatic cartridge for adjusting the temperature. Body and knobs in polished chrome-plated brass. 3-year warranty for the thermostatic cartridge and 10-year warranty for the rest of the fittings. Sanifirst brand thermostatic shower mixer, 150mm span, REF: 75639 or approved equivalent.