75697 - 
Sink one-hole mixer tap with "clic-clac" drainage - deck-mounted model with thin lever. Fixed cast spout with 170.5 mm projection. Spout height: 252 mm. Ø 35 mm ceramic cartridge with energy savings: opening on cold water. Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M10X1, EP G’3/8, Lg 480mm. Basket filter seals mounted on the hoses limiting fouling. Reinforced fixation by a stainless steel rod M8. 10 year warranty. Sanifirst brand single hole washbasin mixer, fixed cast spout REF: 75697 or approved equivalent.