75698 - Washbasin mixer ECO C3 -  Without  drain
One-hole sink mixer tap without "clic-clac" drainage - deck-mounted model with thin lever. Fixed cast spout with 170.5 mm projection. Spout height: 252 mm. Ø 35 mm ceramic cartridge with energy savings: opening on cold water. Flow between 4 and 6L / min at 3 bar - in accordance with the NF standard "medical environment"; possible flow modification, in case of disassembly of the limiters, by adjusting screw between 4 and 20L / min. Cartridge fitted with a mechanical temperature limiting stop allowing adjustment in 5 positions.Tapware fitted as standard star-shaped flow straightener. Body, spout and controls in polished chrome plated brass. SPEX stainless steel braided hoses, M10X1, EP G’3/8, Lg 480mm. Basket filter seals mounted on the hoses limiting fouling. Reinforced fixation by a stainless steel rod M8. 10 year warranty. Sanifirst brand single hole washbasin mixer, fixed cast spout REF: 75698 or approved equivalent.