75715 - 
Single-hole deck-mounted hand-basin mixer tap, MODULMIX design, without drainage for hand-basins, with open-work control. Smooth directional or fixed spout, Len 170mm. Spout height 100mm. Ø 40 pressure balancing ceramic cartridge: temperature limiter, dual flow (hard point at 50% opening). Flow between 10 and 15L / min at 3 bar. Integrated check valves.Tapware fitted with star shaped flow straightener as standard. Smooth body, spout and control component in polished chrome-plated brass. Hoses with SPEX sheath braided stainless steel M10X1, EP G’3/8, Len 350mm. Fixture strengthened using a stainless steel rod. 10 year guarantee. Sanifirst brand type single hole washbasin mixer tap with cast orientable or fixed spout smooth tube REF: 75715 or approved equivalent