75719 - 
Single hole hospital mixer tap (modul’mix design) without drainage for handbasin, with long medical control Len 170mm to avoid hand contact, operated by elbow, forearm or wrist. Fixed or directional, smooth and removable for disinfection Len 250mm. Spout height 100mm. The spout height and length can be adapted without changing the complete tap. Ø 40 ceramic pressure balancing cartridge: temperature limiting stopper with 7 setting positions, dual flow (hard point at 50% opening). Flow between 10 and 15L / min at 3 bar. Integrated check valves. Standard star-shaped tap-nozzle which limits the risk of limescale, eliminates water retention and impurities and is resistant to chlorine and thermal shock treatments. Smooth body, spout and control component in polished chrome-plated brass. Hoses with SPEX sheath braided stainless steel M10X1, EP G’3/8, Len 500mm. Fixture strengthened using a stainless steel rod. 10 year guarantee. Sanifirst brand type single hole pressure balancing hospital mixer tap with removable fixed or directional smooth spout for handbasins REF: 75719 or approved equivalent.