75721 - 
Single-hole deck-mounted sink mixer tap, MODULMIX design, without drainage for hand-basins, with open-work control. Smooth directional or fixed spout, Len 230mm. Spout height 160mm. Ø 40 pressure balancing multi-function ceramic cartridge: temperature limiter, dual flow (hard point at 50% opening). Flow between 10 and 15L / min at 3 ba. Integrated check valves.Tapware fitted with star shaped flow straightener as standard. Body, spout and control component in polished chrome-plated brass. SPEX hoses M10X1, EP G 3/8”, Len 350mm. Fixture strengthened using a stainless steel rod. 10 year guarantee. Sanifirst brand type single hole sink mixer tap with cast directional spout REF: 75721 or approved equivalent.