75723 - 
Sink mixer tap, 150mm span without drainage, wall-mounted with long medical control avoiding hand contact, use with the elbow, forearm or wrist. Extruded directional spout, Len 160mm. Ø 40 multi-function ceramic cartridge: temperature limiting stopper with 7 setting positions, double flow and maximum flow settings. Tapware fitted with star aerator as standard. Body, spout and control component in polished chrome-plated brass. EP G’3/4 connection delivered with base trim and offset M G 1/2” connectors. 10 year guarantee. Sanifirst brand type sink mixer tap, span 150mm with directional extruded spout REF: 75723 or approved equivalent.