75840 - Washbasin mixer - H 100 mm
Washbasin mixer one hole in brass with waste for washbasin, table top with elbow control. Fixed spout Lg 106 mm. Height to nozzle 100 mm. Multifunctional Ø 35
ceramic cartridge: temperature limit stop with 7 setting positions, and maximum flow adjustment. French norm NF Medical environment compliant flow rate (between 4
and 6/min at 3 bar). Original mounted mixer with a star-shaped flow straightener. Body inside and outside smooth (smooth surface in contact with water), polished
spout and actuator . Hoses with braided SPEX sheath stainless steel M10X1, EP G'3 / 8. Fixing with a 1 M8 rod clamping kit. 10 years warranty. Brand Sanifirst type
single lever basin mixer with fixed waste with smooth spout and body REF: 75840 or equivalent approved