75842 - Washbasin mixer - H 100 mm
Washbasin mixer one hole in brass with waste for washbasin, table top with openwork lever. Fixed spout Lg 106 mm. Height to nozzle 100 mm. Multifunctional Ø35 ceramic cartridge: temperature limit stop with 7 setting positions, and maximum flow adjustment. French norm NF Medical environment compliant flow rate (between
4 and 6/min at 3 bar). Original mounted mixer with a star-shaped flow straightener. Body inside and outside smooth (smooth surface in contact with water), polished
spout and actuator. Hoses with braided SPEX sheath stainless steel M10X1, EP G'3/ 8. Fixing with a 1 M8 rod clamping kit. 10 years warranty. Brand Sanifirst type
single lever basin mixer with fixed waste with smooth spout and body REF: 75842 or equivalent approved.