75845 - Washbasin mixer with solid lever without drain - HOPTIM'
Washbasin mixer one hole in brass without drain for washbasin, table top with solid lever. WRAS Approved. Fixed  spout Lg 106 mm. Height to nozzle 100 mm. Multifunctional Ø35 ceramic cartridge: temperature limit stop with 7 setting positions, and maximum flow adjustment. French norm NF Medical environment compliant flow rate (between 4 and 6/min at 3 bar).Original mounted mixer with a star-shaped flow straightener. Body inside and outside smooth (smooth surface in contact with water), polished spout and actuator. Hoses with braided SPEX sheath stainless steel M10X1, EP G'3 / 8. Fixing with a 1 M8 rod clamping kit. 10 years warranty. Brand Sanifirst type single lever basin mixer with smooth spout and body REF: 75845 or equivalent approved.