75873 - Electronic mixer, battery powered, fixed or adjustable  removable nozzle, - Modul'Mix
Electronic battery powered hospital single hole mixer (Modul'Mix design) without drain for hand wash basin, comes with long elbow control for temperature setting. Fixed or swivel spout, smooth and removable for disinfecting L 150mm. Height to nozzle 200mm. Height and length of spout adapted without changing the entire tapware. Multifunctional cartridge: temperature limit stop with 7 positions adjustment; and flow blocked between 4 and 6L / min at 3 bar in accordance with NF "Medical Environment", possible flow modification, in case of disassembly of the limiters, between 4 and 20L / min. Infrared cell integrated in the body, removable without removing the tap.  Power Supply IP65 with 6V lithium battery. Tapware with star-shaped flow straightener  eliminating water retention and impurities; withstands thermal and chlorine shocks Smooth body, spout and controls in polished chrome plated brass. SPEX stainless steel hoses, M10X1, LN G'3 / 8 L 650 mm, filters, solenoid valves and silicon membrane M G'3 / 8. Reinforced fixation by a stainless steel rod. 10 year warranty. Customisable anti-bacteria program (purges, frequency, duration, etc.) Sanifirst Brand electronic hospital single hole mixer with fixed or swivel smooth spout for hand wash basin REF: 75873 or approved equivalent.