75916 - 
Washbasin mixer one hole in brass without waste for washbasin, table top with solid lever. Fixed spout Lg 106 mm. Height to nozzle 100 mm. Energy saving C3 Ø 35 ceramic cartridge: opening on cold water. Cartridge fitted with a mechanical temperature limiter, allowing adjustment. NF "M" compliant flow between 4 and 6L / min at 3 bar. Faucets originally fitted with a star-shaped flow straightener. Smooth interior and exterior body (smooth surface in contact with water), chrome polished spout and operating element. Hoses with stainless steel braided SPEX sheath M10X1, EP G’3 / 8 Fixing by a clamping kit with 1 M8 rod. 10 year warranty. Sanifirst brand type single-hole basin mixer without fixed pop-up waste with smooth spout & body REF: 75916 or equivalent approved