75950 - MASTERMIX thermostatic shower tablet - Downward outlet 
Shower tablet thermostatic mixer without mixing chamber under pressure (avoiding DHW and DCW intercommunication upstream of the shutter), with MASTERMIX conception, equipped with ergonomic swivel knobs, in chrome-plated zamak. Temperature knob with temperature limiter at 41°C. Safety temperature unlocking for thermal shock, and accessible only by technical staff, without dismantling the knob. Connection exclusively by means of a fixing plate with connection MG1/2'' span 150 +/-10mm incorporating filtration and acoustic coupling (supplied).M G ½’’ downward outlet with integrated check valve. Adjustable maximum flow rate 6/9/12 L / min by the technical manager, temperature adjustable from 18° to 41°C. Flow rate knob in chrome-plated zamak. Unique and patented anti-intercommunication hot water (HW) and cold water (CW) system: removal of check valves on the HW and CW mixer inlets. Combination of a compliant French Norm EN1111 thermostatic cartridge and ceramic cartridge. 3-year warranty for thermostatic cartridge and 10-year warranty for the tap. REF: 75950, MASTERMIX technology, brand SANIFIRST or equivalent approved.