75951 - MASTERMIX thermostatic shower tablet - Downward outlet 
Shower thermostatic tablet without mixing chamber under pressure (avoiding DHW and DCW intercommunication upstream of the shutter),with MASTERMIX conception, equipped with ergonomic swivel knob, in chrome-plated zamak, and with TOUCH soft activation button. Temperature knob with temperature limiter at 41°C. Safety temperature unlocking for thermal shock, and accessible only by technical staff, without dismantling the knob. Connection exclusively by means of a fixing plate with connection MG1/2'' span 150 +/- 10mm incorporating filtration and acoustic coupling (supplied).M G ½’’downward outlet with integrated check valve. Opening/closing button with TOUCH technology with default duty flush (30 sec every 24h without use). Fixed flow rate around 8L/min, temperature adjustable from 18° to 41°C. Unique and patented antiintercommunication hot water (HW) and cold water (CW) system: removal of check valves on the HW and CW mixer inlets. Combination of a compliant French Norm EN1111 thermostatic cartridge and two solenoid valves. 3-year warranty for thermostatic cartridge and electronic components and 10-year warranty for the tap. REF: 75951, MASTERMIX technology, brand SANIFIRST or equivalent approve