88816 - Shower panel with single control mixer tap
Shower panel with single lever mixer with ceramic disc(without timed control).
Fixed shower head with adjustable grid and anti-limestone pins.
Maximum temperature internal locking system.
Integrated flow regulator (8 l/min from 1 to 5 bar).
Anodised aluminium finish, high or rear inlet.
Large panel opening without dismantling , fittings on removable plate.