IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
Description: "RevitIdentifiers [VersionGUID: 9afec3e4-8e82-4a76-aeae-fbf6823c1ee5, NumberOfSaves: 0]"
Description: "CoordinateReference [CoordinateBase: Shared Coordinates, ProjectSite: Default Site]"
File name: "18460-presto.ifc"
Time stamp: "2025-06-04T22:53:50"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.80.32 - IFC 22.7.0.0 - Default UI"
Application: "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)"

People and organizations
  Person "mostafa.etmanHDZVT" of Organization (no name given)
  Owner history of Person "mostafa.etmanHDZVT" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1749063228 (2025-06-04T18:53:48Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCDISTRIBUTIONELEMENTTYPE "18460-presto:18460 - presto" | object type "18460-presto:18460 - presto" | names: "18460-presto:18460 - presto:355211" | material: materials ("Silver", "Aluminum 1100-O", "Wall Texture, Orange Peel", "Steel, Paint Finish, GREEN", "Metal, Paint Finish, White, Matte", "Stainless Steel, Polished", "Damp-proofing", "CFRP", "Plastic, Opaque White", "Bronze, Architectural", "<Unnamed>") | property sets: Pset_DistributionFlowElementCommon, Pset_QuantityTakeOff, Constraints, Phasing, Mechanical, Dimensions
      IFCBUILDINGSTOREY "Level 2" | long name "Level 2" | object type "Level:8mm Head" | elevation 4000.0000000000005

Types
  IFCDISTRIBUTIONELEMENTTYPE "18460-presto:18460 - presto" | 1 occurrence | material: materials ("Silver", "Aluminum 1100-O", "Wall Texture, Orange Peel", "Steel, Paint Finish, GREEN", "Metal, Paint Finish, White, Matte", "Stainless Steel, Polished", "Damp-proofing", "CFRP", "Plastic, Opaque White", "Bronze, Architectural", "<Unnamed>") | property sets: Electrical - Loads, Constraints, Mechanical, Materials and Finishes, Identity Data, Other

Property sets
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "18460-presto:18460 - presto" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "18460-presto:18460 - presto" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 2" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 4000.0000000000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Schedule Level = "Level 1" (IFCLABEL)
    Work Plane = "<not associated>" (IFCTEXT)
  Constraints | properties | on 1 type object
    Default Elevation = 1219.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 1.008556760565577 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0057483202797703296 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 2" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Delivered with = "1 Flush valve with stop valve integrated / - 1 Brass coupling nut Male Female 3/4'' (20x27) / - 1 PVC angle tube Ø 32 mm and 1 junction nozzle male 55 mm / - 1 Extended straight PE tube 100 mm with adapter sleeve for connection to the bowl / - 1 WC outlet angle PVC pipe dia. 100 mm / - Screw and dowel for toilet bowl fixing" (IFCTEXT)
    Mark = "2" (IFCTEXT)
    Materials & Finish = "60 micron epoxy coated soldered steel mounting frame / - Galvanized legs and floor fixing plates / - Brass body flush valve / - Anti-vandal brushed stainless steel 304L front plate" (IFCTEXT)
    Operation = "Double flush volume automatic detection depending on the time of user presence (4/6l - short/long detection) / - By pass manual 6l push button (flush can be activated in case of power failure)" (IFCTEXT)
    Power supply = "With mains 7V via 12V / 24V AC or DC. Compatible with 230 V AC / 12 V AC transformer not included ( See Ref. 90464 / 90711/ 90610 / 90685 / 90704 / 90686)" (IFCTEXT)
    Range = "SELF-SUPPORTING MOUTING FRAME WITH DIRECT FLUSH" (IFCTEXT)
    Ref = "18460 - Self-supporting mounting frame with PRESTO 7100 XL N" (IFCTEXT)
    Security = "Patented anti-blocking "S" system preventing the tap to be blocked in open position to avoid continued water flow / - Vacuum breaker device prevents the contamination of the water network from polluted water backflow / - The solenoid valve will be closed automatically in case of low battery or any damage of detector" (IFCTEXT)
    Standards & approvals = "Brass body in accordance with EN 1982, EN 12164, EN 12165 / - 200-hour neutral salt spray resistant (NSS) in accordance with ISO 9227" (IFCTEXT)
    Volume of water delivered = "Small volume: 4l (+/- 1l) Adjustable from 2 to 6l at 2.5 bar / - Large volume: 6l (+/- 1l) Adjustable from 4 to 9l at 2.5 bar / - Volume preset at +/- 1,5l on pressure range from 1,2 to 4 bar / - Anti-water-hammering device / - Automatic 1l/s flow limiter, from 1.2 to 4 bar dynamic working pressure" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "18460" (IFCTEXT)
    Description = "Self-supporting mounting frame with PRESTO 7100 XL N" (IFCTEXT)
    Manufacturer = "presto" (IFCTEXT)
    OmniClass Number = "23.45.00.00" (IFCTEXT)
    OmniClass Title = "Sanitary, Laundry, and Cleaning Equipment" (IFCTEXT)
    Type Name = "18460 - presto" (IFCTEXT)
    URL = "https://www.prestodatashare.com/espacedoc/Fiches_Techniques/GB/18460.pdf" (IFCTEXT)
    brand = "LES ROBINETS PRESTO" (IFCTEXT)
    range = "SELF-SUPPORTING MOUTING FRAME WITH DIRECT FLUSH" (IFCTEXT)
    ref = "18460 - Self-supporting mounting frame with PRESTO 7100 XL N" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "8mm Head" (IFCLABEL)
    Type Id = "305" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "18460-presto" (IFCLABEL)
    Family and Type = "18460-presto: 18460 - presto" (IFCLABEL)
    Type = "18460 - presto" (IFCLABEL)
    Type Id = "355154" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "18460-presto" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    Hydraulic. Supply = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    System Classification = "Sanitary" (IFCTEXT)
    Working Pressure = 499999.99999999994 (IFCPRESSUREMEASURE) [PASCAL]
  Mechanical | properties | on 1 type object
    Recommended pressure = 299999.99999999994 (IFCPRESSUREMEASURE) [PASCAL]
    flow = 6. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    flow time = 1. (IFCTIMEMEASURE) [SECOND]
    min flow = 1. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    min pressure = 99999.999999999985 (IFCPRESSUREMEASURE) [PASCAL]
    pressure = 499999.99999999994 (IFCPRESSUREMEASURE) [PASCAL]
  Constraints(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Other(Type) | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Electrical - Loads | properties | on 1 type object
    power = 0. (IFCPOWERMEASURE) [WATT]
  Materials and Finishes | properties | on 1 type object
    material = "60 micron epoxy coated soldered steel mounting frame / - Galvanized legs and floor fixing plates / - Brass body flush valve / - Anti-vandal brushed stainless steel 304L front plate" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    Manufacturer = "presto" (IFCLABEL)