IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2020-01-22T09:54:16"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (FRA)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (FRA)"

People and organizations
  Person "Polantis_Test" of Organization (no name given)
  Owner history of Person "Polantis_Test" of Organization (no name given) | application "Autodesk Revit 2017 (FRA)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (FRA)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Nom du projet" | phase "Etat du projet"
  IFCSITE "Default" | latitude 48° 52′ 0.117187″ | longitude 2° 19′ 59.880409″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Entrer l'adresse ici", "Paris", "France"
      IFCBUILDINGSTOREY "Niveau 0" | long name "Niveau 0" | elevation -1.94916083273711E-14
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "64652 PRESTO 705 WITH DIRECTIONAL LEVER" | object type "64652 PRESTO 705 WITH DIRECTIONAL LEVER" | names: "PRE050006:64652 PRESTO 705 WITH DIRECTIONAL LEVER:255103" | material: "Polished chrome brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Autre, Contraintes, Cotes, Données d'identification

Types
  IFCVALVETYPE "64652 PRESTO 705 WITH DIRECTIONAL LEVER" | 1 occurrence | material: "Polished chrome brass" | property sets: Autre, Contraintes, Cotes, Données d'identification, Général, Génie climatique

Property sets
  Graphismes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Couleur = 12632256 (IFCINTEGER)
    Epaisseur des lignes = "1" (IFCIDENTIFIER)
    Motif des lignes = "Tiret point" (IFCLABEL)
    Symbole = "Marqueur de niveau - Point triangulaire: Marqueur de niveau - Point triangulaire" (IFCLABEL)
    Valeur par défaut du symbole à l'extrémité 1 = FALSE (IFCBOOLEAN)
    Valeur par défaut du symbole à l'extrémité 2 = TRUE (IFCBOOLEAN)
  Graphismes | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Utiliser l'échelle d'annotations = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Auteur = "" (IFCTEXT)
    Description de l'organisation = "" (IFCTEXT)
    Nom de l'organisation = "" (IFCTEXT)
    Nom du bâtiment = "" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nom du type = "Ligne du Niveau" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Identifiant = "5" (IFCTEXT)
  Données d'identification | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Etage de bâtiment = TRUE (IFCBOOLEAN)
    Nom = "Niveau 0" (IFCTEXT)
    Structure = FALSE (IFCBOOLEAN)
  Données d'identification | properties | on 1 type object
    Code d'assemblage = "" (IFCTEXT)
    Description = "Single deck mounted self-closing tap with multi-directional lever, hot or cold water. Equipped against corrosion and lime scale with a self-cleaning needle and ruby mechanism. Preset at 3L/min (flow rate could be changed by internal device only). Type PRESTO 705 ref 64652 or technically equivalent. NF certified product with 10-year warranty – ISO 90001 manufacturer" (IFCTEXT)
    Description de l'assemblage = "" (IFCTEXT)
    Fabricant = "LES ROBINETS PRESTO S.A." (IFCTEXT)
    Modèle = "64652 PRESTO 705 WITH DIRECTIONAL LEVER" (IFCTEXT)
    Nom de code = "" (IFCTEXT)
    Nom du type = "64652 PRESTO 705 WITH DIRECTIONAL LEVER" (IFCTEXT)
    Numéro OmniClass = "" (IFCTEXT)
    Product data url = "https://bimobject.com/presto/product/PRE050006" (IFCTEXT)
    Titre OmniClass = "" (IFCTEXT)
    URL = "http://www.prestodatashare.com/centretelechargement/index.php?lang=GB&refs=64652" (IFCTEXT)
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base de l'élévation = "Point de base du projet" (IFCIDENTIFIER)
  Contraintes | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Décalage = 0. (IFCLENGTHMEASURE) [METRE]
    Hôte = "Niveau : Niveau 0" (IFCTEXT)
    Niveau = "Niveau: Niveau 0" (IFCLABEL)
  Contraintes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elévation = 0. (IFCLENGTHMEASURE) [METRE]
  Contraintes | properties | on 1 type object
    LC = 0.0225 (IFCLENGTHMEASURE) [METRE]
    PC = 0.0225 (IFCLENGTHMEASURE) [METRE]
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "LES ROBINETS PRESTO S.A." (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "64652" (IFCIDENTIFIER)
  Autre | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Adresse du projet = "Entrer l'adresse ici" (IFCTEXT)
    Catégorie = "Informations sur le projet" (IFCLABEL)
    Date de fin du projet = "Date de fin" (IFCTEXT)
    Etat du projet = "Etat du projet" (IFCTEXT)
    Nom du client = "Propriétaire" (IFCTEXT)
    Nom du projet = "Nom du projet" (IFCTEXT)
    Numéro de projet = "0001" (IFCTEXT)
  Autre | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Catégorie = "Accessoire de canalisation" (IFCLABEL)
    Famille = "PRE050006: 64652 PRESTO 705 WITH DIRECTIONAL LEVER" (IFCLABEL)
    Famille et type = "PRE050006: 64652 PRESTO 705 WITH DIRECTIONAL LEVER" (IFCLABEL)
    ID du type = "PRE050006: 64652 PRESTO 705 WITH DIRECTIONAL LEVER" (IFCLABEL)
    Type = "PRE050006: 64652 PRESTO 705 WITH DIRECTIONAL LEVER" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Famille = "Niveau: Ligne du Niveau" (IFCLABEL)
    Famille et type = "Niveau: Ligne du Niveau" (IFCLABEL)
    ID du type = "Niveau: Ligne du Niveau" (IFCLABEL)
    Type = "Niveau: Ligne du Niveau" (IFCLABEL)
  Autre | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Catégorie = "Niveaux" (IFCLABEL)
    Nom de la famille = "Niveau" (IFCTEXT)
  Autre | properties | on 1 type object
    Catégorie = "Accessoire de canalisation" (IFCLABEL)
    Nom de la famille = "PRE050006" (IFCTEXT)
    Polantis code = "PRE050006" (IFCTEXT)
  Cotes | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Taille = "15 mmø" (IFCTEXT)
    Taille maximale = 0.015 (IFCLENGTHMEASURE) [METRE]
    Taille minimale = 0.015 (IFCLENGTHMEASURE) [METRE]
    Volume = 0.00117647999999994 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Cotes | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Hauteur de calcul = 0. (IFCLENGTHMEASURE) [METRE]
  Cotes | properties | on 1 type object
    Depth = 0.152 (IFCLENGTHMEASURE) [METRE]
    Height = 0.172 (IFCLENGTHMEASURE) [METRE]
    Nominal diameter = 0.015 (IFCLENGTHMEASURE) [METRE]
    Width = 0.045 (IFCLENGTHMEASURE) [METRE]
  Génie climatique | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Abréviation du système = "" (IFCTEXT)
    Classification du système = "Autre" (IFCTEXT)
    Méthode de perte de charge = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    Nom du système = "" (IFCTEXT)
  Génie climatique | properties | on 1 type object
    Flow = 0.00176573333607443 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Loss of load = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Génie climatique - Ecoulement | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Perte de charge = 0. (IFCPRESSUREMEASURE) [PASCAL]
  Isolation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Epaisseur d'isolation = 0. (IFCLENGTHMEASURE) [METRE]
    Taille globale = "15 mmø" (IFCTEXT)
  Phase de construction | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase de création = "Nouvelle construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Général | properties | on 1 type object
    Adress = "7, RUE RACINE - 92542 MONTROUGE CEDEX FRANCE" (IFCTEXT)
    CCTP Link = "http://www.prestodatashare.com/centretelechargement/index.php?lang=GB&refs=64652" (IFCTEXT)
    Connection = "- Male G 1/2" (15x21) cold, hot or pre-mixed water" (IFCTEXT)
    Debit = "3 l/min at 3 bars 4-position setting Anti water-hammer system" (IFCTEXT)
    Edition number = 0 (IFCINTEGER)
    Finish = "Chrome plated brass body High chrome plated fixed spout" (IFCTEXT)
    Function = "Working pressure : - 1 to 5 bar Flow : - 3 l/min at 3 bar - 4-position flow adjustment device - Anti-water-hammering design Flow time : - 15 seconds (± 5 sec.) Operation: - operated through action on the omnidirectional lever control (flexible triggering) Hydraulic supply : - M G 1/2" (15x21) - Cold, hot or premixed water Thermal resistance : - Resistant to a temperature of 75°C for 30-minute-thermal-shocks Security : - Non-removable, wear-proof red or blue marker Delivered with : - 1 Nut for 12x14 tube - 1 Filter gasket - 1 Stainless steel plain washer - 1 Brass clamping nut - 1 Nitrile plain washer - 2 Non-removable, wear-proof coloured marker - Instruction manual Standards & approvals : - Acoustic class II - Brass body in accordance with EN 1982, EN 12164, EN 12165 - Molded chrome-plated body in accordance with EN 12540 - 200-hour neutral salt spray resistant (NSS) in accordance with ISO 9227" (IFCTEXT)
    Instructions for use link = "http://www.prestodatashare.com/centretelechargement/support.php?lang=GB&ref=64652" (IFCTEXT)
    Manufacturer URL = "http://www.prestodatashare.com/centretelechargement/index.php?lang=GB&refs=64652" (IFCTEXT)
    Pressure = "1 to 5 bars" (IFCTEXT)
    Product sheet link = "http://www.prestodatashare.com/espacedoc/Fiches_Techniques/GB/64652.pdf" (IFCTEXT)
    Reference = "64652" (IFCTEXT)
    Variants = "64652" (IFCTEXT)
    Warranty = "10" (IFCTEXT)
  Matériaux et finitions | properties | on 1 type object
    Material = "Polished chrome brass" (IFCLABEL)
  Texte | properties | on 1 type object
    Product Guid = "0f0d0427-0c7c-46eb-8cf8-1de614268743" (IFCTEXT)