14260SB - PRESTO 1000 XL TC Induct mounting - Adapted with rimless toilets bowls 
Flush valve for induct mounting for rimless toilets bowls. Presto 1000 XL TC, ref. 14260SB or technically equivalent. With Water volume adjustable from 2 to 9l. 60l/min flow regulator. The self closing flush valve is equipped with a self-cleaning ruby mechanism and an patented  anti-blocking  ''S''® safety system that prevents blockage in continuous flow. Integrated stop valve and anti-siphonic device. Remote control push button made in Brass chrome plated. 1 Remote control for induct mounting 15 to 200mm with clamping nuts.

14260SB - PRESTO 1000 XL TC Induct mounting - Adapted with rimless toilets bowls 
Flush valve for induct mounting for rimless toilets bowls. Presto 1000 XL TC, ref. 14260SB or technically equivalent. Including : 
- Water volume adjustable from 2 to 9l. 
- 60l/min flow regulator. 
- Self closing flush valve is equipped with a self-cleaning ruby mechanism 
- patented  anti-blocking  ''S''® safety system that prevents blockage in continuous flow
- Integrated stop valve and anti-siphonic device
- Remote control push button made in Brass chrome plated. 
- 1 Remote control for induct mounting 15 to 200mm with clamping nuts.
Included any suggestions for supplies and implementation.