14301SB - PRESTO 1000 XL A DVA - Adapted with rimless toilets bowls 
Double volume concealed direct flush valve with adjustable volumes for rimless toilet bowl. Presto 1000 XL A DVA® ref. 14301SB or technically equivalent
Water volume delivered from 6 to 9 liters (for high volume) adjustable with wrench,
And from 2.5 to 5 liters (Low volume) adjustable by the slider on front plate.
60l/min flow regulator.
The self closing Flush valve is equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow.
The front plate is bright chromed with double button for 2 different flush volumes.
Integrated stop valve valve and anti-vacuum (anti-siphonic) device. 

14301SB - PRESTO 1000 XL A DVA - Adapted with rimless toilets bowls 
Double volume concealed direct flush valve with adjustable volumes for rimless toilet bowl. Presto 1000 XL A DVA® ref. 14301SB or technically equivalent. Including :
- Water volume delivered from 6 to 9 liters (for high volume) adjustable with wrench,
- And from 2.5 to 5 liters (Low volume) adjustable by the slider on front plate.
- 60l/min flow regulator.
- The self closing Flush valve is equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow.
- The front plate is bright chromed with double button for 2 different flush volumes.
- Integrated stop valve valve and anti-vacuum (anti-siphonic) device. 
Included any suggestions for supplies and implementation. 

PRODUCT ASSOCIATES
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting