14303SB - PRESTO 1000 XL E DVA ECO 2L/4L - Adapted with rimless toilets bowls 
Double volume concealed direct flush valve with adjustable volumes for rimless toilet bowl. Type Presto P1000 XL E DVA ECO réf. 14303SB or technically equivalent. With a double water volume delivered of 4l for large flush and 2l for small flush, adjustable with wrench. 60l/min flow regulator. The self closing flush valve is equipped with a self-cleaning ruby mechanism and an S® safety system that prevents blockage in continuous flow. The front plate is chrome brushed with double button for 2 different flush volumes. Integrated stop valve valve and anti-vacuum (anti-siphonic) device. 

14303SB - PRESTO 1000 XL E DVA ECO 2L/4L - Adapted with rimless toilets bowls 
Double volume concealed direct flush valve with adjustable volumes for rimless toilet bowl. Type Presto P1000 XL E DVA ECO réf. 14303SB or technically equivalent. Including : 
- a double water volume delivered of 4l for large flush and 2l for small flush, adjustable with wrench
- 60l/min flow regulator
- a self-cleaning ruby mechanism 
- an S® safety system that prevents blockage in continuous flow
- a chrome brushed front plate with double button for 2 different flush volumes
- integrated stop valve valve and anti-vacuum (anti-siphonic) device
Included any suggestions for supplies and implementation. 

RELATED PRODUCTS
Ref. 47850 Angled pipe in diameter 28mm PVC and in 4 glue-together parts - channel of diameter 55
Ref. 47681 Counter-angled pipe in diameter 28mm PVC for concealed mouting