57038 - PRESTO NEO Sensor deck-mounted  - Power Supply
Deck mounted single tap with detection (CE). Presto NEO® SENSOR type ref. 57038 or technically equivalent. With optoelectronic sensor cell, 230 V AC/DC transformer power supply. Built-in flow regulator (1.9 l / min). Anti-lock system prevents continuous flow. High quality anti limescale Spayer.

57038 - PRESTO NEO Sensor deck-mounted  - Power Supply
Deck mounted single tap with detection (CE). Presto NEO® SENSOR type ref. 57038 or technically equivalent including:
- optoelectronic sensor cell, 
- 230 V AC/DC transformer power supply. 
- Built-in flow regulator (1.9 l / min).
-  Anti-lock system prevents continuous flow.
- High quality anti limescale Spayer.