57202NP - Deck-mounted sensor single tap for washbasin, mains 12-24V, 1.9l/min without stop valve Polished Black
Deck-mounted sensor single tap for washbasin Presto LINEA® ref 57202NP or technically equivalent. Touchless trigger, suitable for PRM. Flow 1.9l/min with integrated regulated flow spray. Mains-operated without transformer for low voltage power supply (12-24V AC/DC). Integrated solenoid valve. F G 3/8" (12x17) hose connection. Anti-overflow security time set to 30 seconds. Adjustable duty flush of 30 sec every 24h after last use. Polished Black finish. Delivered with PEX hose, filter gaskets.

57202NP - Deck-mounted sensor single tap for washbasin, mains 12-24V, 1.9l/min without stop valve Polished Black
Deck-mounted sensor single tap for washbasin Presto LINEA® ref 57202NP or technically equivalent. 
- Touchless trigger, suitable for PRM
- Flow 1.9l/min with integrated regulated flow spray
- Mains-operated without transformer for low voltage power supply (12-24V AC/DC)
- Integrated solenoid valve
- F G 3/8" (12x17) hose connection
- Anti-overflow security time set to 30 seconds
- Adjustable duty flush of 30 sec every 24h after last use 
- Polished Black finish
- Delivered with PEX hose, filter gaskets