57280 - Deck-mounted sensitive mixer tap, battery ,1,9l/min, 7 sec
Single touch/sensitive (CE) deck-mounted tap, timed (1s to 5min), for cold or mixed water supply. PRM-compatible Presto LINEA TOUCH® type tap, ref. 57280 or technically equivalent. Features touch start/stop function and integrated flow regulator (1,9l/min). Brass body with Chrome finish. Powered by Integrated 3V CR123A lithium batteries (x2). Includes PEX flexibles. Configurable automatic purge.

57280 - Deck-mounted sensitive mixer tap, battery ,1,9l/min, 7 sec
Single touch/sensitive (CE) timed tap (1s to 5min) on deck, for cold or mixed water supply. PRM-compatible Presto LINEA TOUCH® type tap, ref. 57280 or technically equivalent, includes:
-Touch start/stop function
-Integrated flow regulator at 1,9l/min
-Brass body with Chrome finish
- Powered by Integrated 3V CR123A lithium batteries (x2)
-A PEX flexible
-Configurable automatic purge.
-Includes all supply and installation suggestions.